1. Connect a Dynaflex to the PC the update is being performed from
2. Download the update package from <https://www.dropbox.com/scl/fi/w9gxez3fafoszg2dpjd01/Dynaflex-Contactless-Limit-Update.zip?rlkey=egc0h11t5prducsgqlfpckmba&st=md59a2wo&dl=0>
3. Extract the “Dynaflex Contactless Limit Update” folder
4. Enter the extracted folder
5. Enter the “DynaFlex Utility” folder
6. Run the file “DynaFlexUtility.exe”
7. Click on the connect button at the top of the utility (Green + with a plug icon)
8. Click on the “Settings” tab
9. Click on “EMV / SRED” on the left of the screen
10. On the right side of the screen, click on the drop-down associated with “EMV Property:” and select “Config – Excel”
11. Click on “Send File…”
12. Select the “ContactlessLimitUpdate\_CFG0006364-G0.xlsx” file from the package downloaded in step 2
13. Utility will display “Converting Data…” at the bottom of the window
14. Once the update is complete, a message stating “SUCCESSFULLY Sending Config data to Device” will appear. Click OK on this window
15. Close the Dynaflex Utility window